# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of 3 minibuses to the Kosovo Specialist Chambers**

**p 1 /…**

**Publication reference:** KSCR/PROC/2021-2023/0878

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

**Technical Specifications for 8+1 Seater Mini Bus Vehicle**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications available in catalogue, and/or stock/on order (YES/NO)** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| **Supply of three 8+1 Seater Mini Bus Vehicles**  **(Mananufacturers and models that would fall under this vehicle type: Fiat Talento, Ford Transit, Volkswagen Transporter, Renault Trafic, Mercedes Benz Vito, Toyota PROACE, Opel Vivaro, or equivalent. This list serves only to define the type of vehicle sought, and should not be seen as exhaustive.) When preseting their technical specifications, bidders are encouraged not to make reference to any brands unless necessary for the protection of patents/intelectual property.**   1. **Overall Objective**   This vehicle is to be used to transport up to 8 people plus 1 driver and equipment on all types of roads, predominantly on tarmac/paved/mettlaled (asphalt) road in an urban context.   1. **Purpose**   The purpose of this contract is as follows:   * Supply of 8+1 Seater Mini Bus Vehicles to be used in all weather conditions, on tarmac/paved/mettaled roads, generally parked outdoors, therefore exposed to the elements. The offered Vehicle **must** be in compliance with all mandatory requirements. | |  |  |  |

| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications available in catalogue, and/or stock/on order (YES/NO)** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1. Minimum Mandatory Requirements),** the vehicles supplied **must** meet the following criteria**:** | | | | |
| **1.1** | **General:** The vehicles supplied **must** meet the following criterias:  **Condition:** New/unused, of the most recent models and incorporating all recent improvements in design and materials;  **Manufacturing Date:** Within the last 12 months from order date;  **Drive:** Available as Left Hand Drive version;  **Windows:** Clear windows;  **Vehicle Exterior Colours:** Standard colours of choice to be included in the price;  **Vehicle Interior:** Dark (e.g. dark grey, anthracite or black), seat material to be cleanable dark colour (e.g. dark grey, anthracite or black) textile material;  **Number of Seats:** 8 passengers + 1 driver (back seats removable);  **Payload:** Minimum 1000 kg which envisages maximum number persons + equipment; Speed sensitive and power assisted steering and braking system; | **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO** |  |  |
| **1.2** | **Engine:**  **Fuel Type:** Diesel or Petrol (No hybrid engines);  **Engine Displacement:** Minimum 1.6 l;  **Power:** Minimum power 80 kW;  **Emission:** Meet or exceed the prevailing CO₂emission performance standards within the European Union; | **YES NO**  **YES NO**  **YES NO**  **YES NO** |  |  |
| **1.3** | **Body:**  **Type**: Mini Bus;  **Ground Clearance**: Minimum 150 mm;  **Cabin Doors:** Minimum 4;  **Maximum Length:** 5350 mm; | **YES NO**  **YES NO**  **YES NO**  **YES NO** |  |  |
| **1.4** | **Transmission:**  Two wheel drive (2x4),  Manual Transmission;  Minimum 5 speed forward; | **YES NO**  **YES NO**  **YES NO** |  |  |
| **1.5** | **Wheels:** |  |  |  |
|  | Minimum 16" maximum 17" with all season (M+S type plus Snowflake) street tyre tread pattern, the speed index and load rating of the tyre must be conform with the maximum speed and GVW of the vehicle;  Spare Wheel: Full Size identical to the fitted wheels;  Wheel locks (anti-theft); | **YES NO**  **YES NO**  **YES NO** |  |  |
| **1.6** | **Safety:**  Airbags: Front for driver and passenger;  Seat Belts (3 point) for all passenger seats;  ABS Braking System;  Traction Control System;  Vehicle Stability System;  Acoustic seat belt reminder; | **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO** |  |  |
| **1.7** | **On Board Equipment:**  First Aid Kit (European Standard, DIN 13164 (2014-01) or equivalent);  Warning triangle, two (2) per vehicle;  High visibility vests, one (1) per seat;  Fire extinguisher two (2) per vehicle (1 kg weight, refillable, metal body) Class A B C (one fire extinguisher in the passenger compartment and one in rear) with fitting brackets;  Set of spare light bulbs (for all external lamps, where applicable); Wheel nut wrench;  Set of basic on-board tools;  Jack (suitable to vehicle weight and height);  Box or heavy duty carrying bag containing the above listed items; | **YES NO** |  |  |
| **1.8** | **Vehicle Documents:**  Full set of manuals and documentation (i.e. user manual, service book and all other standard and/or relevant documents) to be provided;  n/a | **YES NO** |  |  |
| **1.9** | **Miscellaneous Requirements:**  Parking Sensors (front and rear);  Rubber Floor Mat Set Heavy Duty Type (front and rear seats);  Air Conditioning;  Remote controlled central locking system;  Internal independent manual door opening override to all doors;  Powered exterior mirrors;  AM/FM Radio;  Bluetooth connectivity to cellular phone; 12 V access point + minumum 1nr. USB socket;  Anti-tamper fuel filler cap or equivalent integrated mechanism;  Fuel system sediment trap;  Dust/Pollen/Cabin filter;  Anti-theft warning system/Immobiliser;  Maintenance free vehicle battery;  Front and rear towing eyes or hooks;  Warranty period: minumum 24 months from the date of the provisional acceptance | **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO**  **YES NO** |  |  |